
	STAR LC 10 CCL printer commands
	(epson compatible)

 code
 (0x07-0x1a)
 7			Bell
 8			ASCII: Backspace
 8 m1 m2 ... 14/15	CBM: Print single-density 7-bit graphics
 9			ASCII: TAB
 9 m1 m2 ... 14/15	CBM: Print double-density 7-bit graphics
 10			LF
 11			Vertical Tab
 12			FF
 13			CR
 14			CBM: Expanded printing
 14			ASCII: Expanded printing for one line
 15			CBM: Cancel expanded printing
 15			ASCII: Condensed printing for one line
 16 n1 n2		Absolute horizontal tab in columns
 17			CBM: Select business character set
 18			ASCII: Cancel condensed printing
 18			CBM: Reverse printing
 19			Cancel top and bottom margins
 20			ASCII: Cancel one-line expanded printing
 26			CBM: Repeat 7-bit graphics pattern

 27  10			Reverse line feed
 27  12			Return to top of current page
 27  15			Condensed printing
 27  16 n1 n2		Absolute horizontal tab in inches
 27  18 m1 m2 ... 14	Print reverse single-density 7-bit graphics
 27  25  0		Manual feed
 27  25  4		Auto feed
 27  25 82		Eject paper from ASF
 27  25 84 n		Set print start position on ASF
 27  33  n		Select master print mode
 27  37 48		Select ROM character set
 27  37 49		Select download character set

 27  38 0 n1 n2 m0 m1 ... m46	Define NLQ download characters
 27  38 0 n1 n2 m0 m1 ... m11	Define draft download characters
 27  42 n0 n1 n2 m1 m2 ...	Select graphics mode

 27  43 ... 30		Define macro instruction
 27  43  1		Execute macro instruction
 27  45 48		Stop underlining
 27  45 49		Start underlining
 27  48			Set line spacing to 1/8 inch (27/216)
 27  49			Set line spacing to 7/72 inch (21/216)
 27  50			Set line spacing to 1/6 inch (36/216, (4,2mm) default)
 27  51 n		Set line spacing to n/216 inch
 27  52			Select italic characters
 27  53			Select upright characters
 27  58 0 0 0		Copy standard characters from ROM into RAM
 27  64			Reset printer
 27  65 n		Set line spacing to n/72 inch
 27  66 n1 n2 ... 0	Set vertical tab stops
 27  67 0  n		Set page length to n inches
 27  67 n		Set page length to n lines
 27  68			ASCII: Set horizontal tab stops
 27  69			Emphasized printing
 27  70			Cancel emphasized printing
 27  71			Double-strike printing
 27  72			Cancel double-strike printing
 27  74  n		Perform one n/216-inch line feed
 27  75 n1 n2 m1 m2 ...	Print single-density 8-bit graphics
 27  76 n1 n2 m1 m2 ...	Print double-density 8-bit graphics
 27  77			Elite pitch
 27  78  n		Set bottom margin
 27  79			Cancel top and bottom margins
 27  80			Pica pitch
 27  81  n		Set right margin
 27  82  n		Select international character set
 27  83 48		Superscript
 27  83 49		Subscript
 27  84			Cancel superscript or subscript
 27  87 48		Cancel expanded printing
 27  87 49		Expanded printing
 27  89 n1 n2 m1 m2 ...	Print double-density, double-speed 8-bit graphics
 27  90 n1 n2 m1 m2 ...	Print quadruple-density 8-bit graphics
 27  93 48		Select Commodore operating mode
 27  93 49		Select ASCII operating mode
 27  97  0		Left justify
 27  97  1		Center text
 27  97  2		Right justify
 27  97 48		Left justify
 27  97 49		Center text
 27  97 50		Right justify
 27  99  n		Set top margin
 27 104  n		Select double or quadruple size
 27 107  n		Select NLQ type style
 27 108  n		Set left margin
 27 112 48		Select fixed spacing
 27 112 49		Select proportional spacing
 27 114  n		Select printing colour
 27 119 48		Return to normal height
 27 119 49		Print double-height characters
 27 120 48		Select draft quality characters
 27 120 49		Select NLQ characters
 27 126 48		Select normal zero
 27 126 49		Select slash zero

 40 40 48 41 41		((0))	Manual feed
 40 40 52 41 41		((4))	Auto feed
 40 40 66 41 41 0	((B))	Cancel double-strike printing
 40 40 66 41 41 1	((B))	Double-strike printing
 40 40 67 41 41 n	((C))n	Select printing colour
 40 40 70 41 41 n	((F))n	Select type style
 40 40 73 41 41 0	((I))0	Select upright characters
 40 40 73 41 41 1	((I))1	Select italic characters
 40 40 82 41 41		((R))	Eject paper from ASF
 40 40 83 41 41 n	((S))n	Select character size
 40 40 84 41 41 n	((T))n	Set print start position on ASF

 (0x91-0x93)
 145			CBM: Select graphics character set
 146			CBM: Cancel reverse printing
 147			Set six-line bottom margin

