ARES_GETNAMEINFO(3)

NAME
ares_getnameinfo - Address-to-nodename translation in protocol-independent manner

SYNOPSIS
#include <ares.h>

typedef void (*ares_nameinfo_callback)(void *arg, int status,
char *node, char *service)

void ares_getnameinfo(ares_channel channel, const struct sockaddr *sa,
socklen_t salen, int flags, ares_nameinfo_callback callback,
void *arg)

DESCRIPTION
The ares_getnameinfo function is defined for protocol-independent address translation. The function is a combination of ares_gethostbyaddr(3) and getservbyport(3). The function will translate the address either by executing a host query on the name service channel identified by channel or it will attempt to resolve it locally if possible. The parameters sa and len give the address as a sockaddr structure, and flags gives the options that the function will use. Valid flags are listed below:

ARES_NI_NOFQDN
    Only the nodename portion of the FQDN is returned for local hosts.

ARES_NI_NUMERICHOST
    The numeric form of the hostname is returned rather than the name.

ARES_NI_NAMEREQD
    An error is returned if the hostname cannot be found in the DNS.

ARES_NI_NUMERICSERV
    The numeric form of the service is returned rather than the name.

ARES_NI_TCP
    The service name is to be looked up for the TCP protocol.

ARES_NI_UDP
    The service name is to be looked up for the UDP protocol.

ARES_NI_SCTP
    The service name is to be looked up for the SCTP protocol.

ARES_NI_DCCP
    The service name is to be looked up for the DCCP protocol.

ARES_NI_NUMERICSCOPE
    The numeric form of the scope ID is returned rather than the name.

ARES_NI_LOOKUPHOST
    A hostname lookup is being requested.

ARES_NI_LOOKUPSERVICE
    A service name lookup is being requested.

When the query is complete or has failed, the ares library will invoke callback. Completion or failure of the query may happen immediately, or may happen during a later call to ares_process(3), ares_destroy(3) or ares_cancel(3).

The callback argument arg is copied from the ares_getnameinfo argument arg. The callback argument status indicates whether the query succeeded and, if not, how it failed. It may have any of the following values:

ARES_SUCCESS
    The host lookup completed successfully.

ARES_ENOTIMP
    The ares library does not know how to look up addresses of type family.

ARES_ENOTFOUND
    The address addr was not found.

ARES_ENOMEM
    Memory was exhausted.

ARES_EDESTRUCTION
    The name service channel channel is being destroyed; the query will not be completed.

ARES_EBADFLAGS
    The flags parameter contains an illegal value.

On successful completion of the query, the callback argument node contains a string representing the hostname (assuming ARES_NI_LOOKUPHOST was specified). Additionally, service contains a string representing the service name (assuming ARES_NI_LOOKUPSERVICE was specified). If the query did not complete successfully, or one of the values was not requested, node or service will be NULL.

SEE ALSO
ares_process(3), ares_getaddrinfo(3)

AUTHOR
Dominick Meglio
Copyright 2005 by Dominick Meglio.